# This file was generated using idf.py save-defconfig. It can be edited manually.
# Espressif IoT Development Framework (ESP-IDF) 5.5.1 Project Minimal Configuration
#
CONFIG_BOARD_TYPE_M5STACK_CORE_TAB5=y

CONFIG_XIAOZHI_ENABLE_ROTATE_CAMERA_IMAGE=y
CONFIG_CAMERA_SC202CS=y

CONFIG_ESP_HOSTED_PRIV_SDIO_PIN_CMD_SLOT_1=13
CONFIG_ESP_HOSTED_PRIV_SDIO_PIN_CLK_SLOT_1=12
CONFIG_ESP_HOSTED_PRIV_SDIO_PIN_D0_SLOT_1=11
CONFIG_ESP_HOSTED_PRIV_SDIO_PIN_D1_4BIT_BUS_SLOT_1=10
CONFIG_ESP_HOSTED_PRIV_SDIO_PIN_D2_4BIT_BUS_SLOT_1=9
CONFIG_ESP_HOSTED_PRIV_SDIO_PIN_D3_4BIT_BUS_SLOT_1=8
